




Model




Modified exit of the CV on magnet supply line






Expansion loads

186 MPa < fa (225 MPa)



Sustained loads

16 MPa < fh (133 MPa)





Pressure test

60 MPa < ftest (207 MPa)



FB 11 deg R





9,75 deg L

